

# One owner, low-time Ovation with two years of warranty remaining.

# Gorgeous paint and interior design!

#

# STATUS

# Airframe, total time: 100 hours

* Engine: 100 hours
* Propeller: 100 hours
* Annual: April 2020

# PERFORMANCE

# Max cruise: 197 KTAS

# Rate of climb: 1,300 fpm at sea level and max weight

# Max range (standard tanks): 1,800 nm (102 U.S. gallons)

# Max range (long-range tanks): 2,400 nm (130 U.S. gallons)

# Max operating altitude: 20,000 feet

# Take-off roll: 1,380 (sea level, max weight)

# ENGINE

* Continental IO-550-G, 310 HP
gold standard engine with three-year warranty (parts and labor)

# PROPELLER

* Hartzell three-blade constant speed

# EXTERIOR/INTERIOR

* Exterior trim: Snow White, Blue Breeze Pearl and Silver Illusion Pearl striping
* Interior: all gray leather interior with black accents and carpet
* Executive interior with tinted aft windows
* AmSafe seatbelts: pilot and copilot

AVIONICS

* Garmin NXI integrated avionics with Jepp charts and SafeTaxi™
* Dual WAAS GPS approach and enroute
* Synthetic vision
* Terrain warning
* GDL69A SXM radio and weather
* Flight Stream 510 – Bluetooth to iPads
* MFD charts — on-screen IFR/VFR charts
* Vertical nav enroute and approach
* GFC 700 digital approach couple autopilot with FD
* GDU 1054, 10” Primary Flight Display, three-axis flight dynamics, air speed, altitude, VS, HSI with perspective modes
* GDU 1054, 10” Multi-Function Display
* GDC 72 Integrated Digital Air Data Computer, constant display of TAS CAS, wind direction, VSI and TAT
* GRS 79 Solid-State Attitude and Heading Reference System
* Dual GIA63W, integrated radio modules with IFR-approved WAAS GPS, VHF navigation with ILS and VHF communication with 16-watt 8.33-KHZ transceivers
* GMA 1347 Digital Audio Controller with integrated marker beacon and intercom
* GTX 345R Integrated Mode-S Transponder with traffic and WX info service and ADS-B in and out
* GEA 71 Airframe/Engine Interface Unit
* GMU 44 Magnetometer
* Artex ME406 ELT
* Stand-by instrumentation: mid-continent SAM-MD302 two-inch standby attitude module, compass with emergency lighting
* Bose headsets series A20 – pilot and copilot

**STANDARD AIRFRAME OPTIONS**

* Redundant dual dc electrical bus
* Dual alternators and batteries
* 1.5-inch rudder pedal extensions
* Xenon landing and taxi lights
* Standby alternator, dual bus system

**ADDITIONAL EQUIPMENT**

* Air conditioning
* Precise Flight Oxygen System (77.1 cubic foot)



